SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Macros | Functions
IL9163/ST7735: il9163/st7735 control functions

## Macros
#define | st7735_setRotation il9163_setRotation
| Sets screen orientation (rotation) More...

## Functions
void | il9163_setRotation (uint8_t rotation)
| Sets screen orientation (rotation) More...

## Detailed Description

## Macro Definition Documentation

## ◆ st7735_setRotation

#define st7735_setRotation il9163_setRotation

Sets screen orientation (rotation)

Sets screen orientation (rotation): 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Parameters

  rotation | - screen rotation 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Note
  works only with ST7735 display

Definition at line 124 of file lcd_il9163.h.

## Function Documentation

## ◆ il9163_setRotation()

void il9163_setRotation | ( | uint8_t | rotation | ) |

Sets screen orientation (rotation)

Sets screen orientation (rotation): 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Parameters

  rotation | - screen rotation 0 - normal, 1 - 90 CW, 2 - 180 CW, 3 - 270 CW

Note
  works only with IL9163 display

Definition at line 263 of file lcd_il9163.c.