SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Enumerations
ssd1331_commands.h File Reference

Go to the source code of this file.

## Enumerations
enum | ESsd1331Commands { SSD1331_COLUMNADDR = 0x15, SSD1331_DRAWLINE = 0x21, SSD1331_ROWADDR = 0x75, SSD1331_CONTRASTA = 0x81, SSD1331_CONTRASTB = 0x82, SSD1331_CONTRASTC = 0x83, SSD1331_MASTERCURRENT = 0x87, SSD1331_PRECHARGEA = 0x8A, SSD1331_PRECHARGEB = 0x8B, SSD1331_SEGREMAP = 0xA0, SSD1331_SETSTARTLINE = 0xA1, SSD1331_SETDISPLAYOFFSET = 0xA2, SSD1331_NORMALDISPLAY = 0xA4, SSD1331_SETMULTIPLEX = 0xA8, SSD1331_SETMASTER = 0xAD, SSD1331_DISPLAYOFF = 0xAE, SSD1331_DISPLAYON = 0xAF, SSD1331_POWERMODE = 0xB0, SSD1331_SETPRECHARGE = 0xB1, SSD1331_CLOCKDIV = 0xB3, SSD1331_PRECHARGELEVEL = 0xBB, SSD1331_VCOMH = 0xBE, SSD1331_NOP = 0xE3 }

## Detailed Description

SSD1331 commands definitions

Definition in file ssd1331_commands.h.

## Enumeration Type Documentation

## ◆ ESsd1331Commands

enum ESsd1331Commands

SSD1331 LCD driver commands

Definition at line 37 of file ssd1331_commands.h.