SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Functions
vga.h File Reference
`#include "ssd1306_hal/io.h"`

Go to the source code of this file.

## Functions
void | ssd1306_vga_delay (uint32_t ms)
void | ssd1306_debug_print_vga_buffer (void(*func)(uint8_t))

## Detailed Description

VGA basic data. Do not include this header in your project!!!

Definition in file vga.h.

## Function Documentation

## ◆ ssd1306_debug_print_vga_buffer()

void ssd1306_debug_print_vga_buffer | ( | void(*)(uint8_t) | func | ) |

Prints vga buffer in text form using passed callback

Parameters

  func | callback to use for printing single character

## ◆ ssd1306_vga_delay()

void ssd1306_vga_delay | ( | uint32_t | ms | ) |

Make ms milliseconds delay. This function has very low precision: 16ms.

Parameters

  ms | time in milliseconds