SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Functions
DIRECT DRAW: 16-bit API functions only for color displays

LCD direct draw functions only for color display. More...

## Functions
void | ssd1306_drawBufferFast16 (lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *data)

## Detailed Description

LCD direct draw functions only for color display.

LCD direct draw functions are applicable for color display types. These functions will NOT work in ssd1306 compatible mode. Use ssd1306_setMode() function to change display mode to NORMAL. You can combine combine NanoEngine capabilities with these functions. Direct draw functions draw directly in GDRAM and do not use any double-buffering.

## Function Documentation

## ◆ ssd1306_drawBufferFast16()

void ssd1306_drawBufferFast16 | ( | lcdint_t | x,
|  | lcdint_t | y,
|  | lcduint_t | w,
|  | lcduint_t | h,
|  | const uint8_t * | data
| ) |  |

Draws 16-bit bitmap, located in SRAM, on the display Each byte represents separate pixel: refer to RGB_COLOR16 to understand RGB scheme, being used.

Parameters

  x | - horizontal position in pixels
  y | - vertical position in pixels
  w | - width of bitmap in pixels
  h | - height of bitmap in pixels
  data | - pointer to data, located in SRAM.

Definition at line 30 of file ssd1306_16bit.c.