SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

io.h
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
24
25 /*
26 * @file hal/arduino/io.h SSD1306 ARDUINO IO communication functions
27 */
28
29 #ifndef _SSD1306_ARDUINO_IO_H_
30 #define _SSD1306_ARDUINO_IO_H_
31
32 #if defined(ARDUINO_ARCH_STM32) // stm32duino support
33 #include <Arduino.h>
34 #include <avr/pgmspace.h>
35 #elif defined(ESP8266) || defined(ESP32) || defined(ESP31B) // esp arduino support
36 #include <Arduino.h>
37 #include <pgmspace.h>
38 #else // AVR support
39 #include <Arduino.h>
40 #include <avr/pgmspace.h>
41 #include <avr/interrupt.h>
42 #if !defined(ARDUINO_ARCH_SAMD) && defined(__AVR__)
43 #include <avr/sleep.h>
44 #endif
45 #endif
46
47 #if defined(ARDUINO_ARCH_STM32)
48
49 #define CONFIG_PLATFORM_I2C_AVAILABLE
50
51 #define SSD1306_WIRE_CLOCK_CONFIGURABLE
52
53 #define CONFIG_PLATFORM_SPI_AVAILABLE
54
55 #define CONFIG_STM32_I2C_AVAILABLE
56
57 #elif defined(ARDUINO_AVR_DIGISPARK) || defined(ARDUINO_AVR_DIGISPARKPRO)
58
59 #define CONFIG_PLATFORM_I2C_AVAILABLE
60 #if defined(ARDUINO_AVR_DIGISPARKPRO)
61
62 #define CONFIG_PLATFORM_SPI_AVAILABLE
63 #else
64
65 #define CONFIG_SOFTWARE_I2C_AVAILABLE
66 /* Define lcdint as smallest types to reduce memo usage on tiny controllers. *
67 * Remember, that this can cause issues with large lcd displays, i.e. 320x240*/
68 #define LCDINT_TYPES_DEFINED
69 typedef int8_t lcdint_t;
70 typedef uint8_t lcduint_t;
71 #endif
72
73 #elif defined(ARDUINO_AVR_ATTINYX5)
74
76 #define CONFIG_SOFTWARE_I2C_AVAILABLE
77
78 #define CONFIG_PLATFORM_I2C_AVAILABLE
79
80 #define CONFIG_USI_SPI_AVAILABLE
81
82 #define CONFIG_PLATFORM_SPI_AVAILABLE
83
85 #define LCDINT_TYPES_DEFINED
86
87 typedef int8_t lcdint_t;
89 typedef uint8_t lcduint_t;
91 #define CONFIG_MULTIPLICATION_NOT_SUPPORTED
92
93 #elif defined(__AVR_ATtiny25__) || defined(__AVR_ATtiny45__) || defined(__AVR_ATtiny85__) || \
94 defined(__AVR_ATtiny24__) || defined(__AVR_ATtiny44__) || defined(__AVR_ATtiny84__)
95
97 #define CONFIG_SOFTWARE_I2C_AVAILABLE
98
99 #define CONFIG_USI_SPI_AVAILABLE
100
102 #define LCDINT_TYPES_DEFINED
103
104 typedef int8_t lcdint_t;
106 typedef uint8_t lcduint_t;
108 #define CONFIG_MULTIPLICATION_NOT_SUPPORTED
109
110 #elif defined(ESP8266) || defined(ESP32) || defined(ESP31B) || defined(ARDUINO_ARCH_SAMD)
111 /* SW implementation of i2c isn't supported on ESP platforms */
113 #define CONFIG_PLATFORM_I2C_AVAILABLE
114
115 #define SSD1306_WIRE_CLOCK_CONFIGURABLE
116
117 #define CONFIG_PLATFORM_SPI_AVAILABLE
118
119 #elif defined(__AVR_ATmega328P__)
120
121 #define CONFIG_SOFTWARE_I2C_AVAILABLE
122
123 #define CONFIG_PLATFORM_I2C_AVAILABLE
124
125 #define SSD1306_WIRE_CLOCK_CONFIGURABLE
126
127 #define CONFIG_TWI_I2C_AVAILABLE
128
129 #define CONFIG_PLATFORM_SPI_AVAILABLE
130
131 #define CONFIG_AVR_SPI_AVAILABLE
132
133 #define CONFIG_AVR_UART_AVAILABLE
134
135 #define CONFIG_VGA_AVAILABLE
136
137 #elif defined(NRF52) || defined(NRF5)
138
139 #define CONFIG_PLATFORM_I2C_AVAILABLE
140
141 #define SSD1306_WIRE_CLOCK_CONFIGURABLE
142
143 #define CONFIG_PLATFORM_SPI_AVAILABLE
144
145 #else
146
147 #define CONFIG_SOFTWARE_I2C_AVAILABLE
148
149 #define CONFIG_PLATFORM_I2C_AVAILABLE
150
151 #define SSD1306_WIRE_CLOCK_CONFIGURABLE
152
153 #define CONFIG_TWI_I2C_AVAILABLE
154
155 #define CONFIG_PLATFORM_SPI_AVAILABLE
156
157 #define CONFIG_AVR_SPI_AVAILABLE
158 #endif
159
160 //#ifdef CONFIG_PLATFORM_I2C_AVAILABLE
161 //#ifdef __cplusplus
162 //#include <Wire.h>
163 //#endif
164 //#endif
165
166 #endif // _SSD1306_ARDUINO_IO_H_
167
lcdint_t
int lcdint_t
Definition: io.h:63
lcduint_t
unsigned int lcduint_t
Definition: io.h:65