SSD1306 OLED display driver 1.7.8 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Classes | Macros | Typedefs | Enumerations
nano_gfx_types.h File Reference
`#include "ssd1306_hal/io.h"`

Go to the source code of this file.

## Classes
struct | SFontHeaderRecord
struct | SUnicodeBlockRecord
struct | SFixedFontInfo
struct | SCharInfo
struct | SSD1306_RECT
struct | SPRITE

## Macros
#define | min(a, b) ((a)<(b)?(a):(b))
#define | max(a, b) ((a)>(b)?(a):(b))
#define | RGB_COLOR8(r, g, b) ( (r & 0xE0) | ((g >> 3)&0x1C) | (b>>6) )
#define | RGB_COLOR16(r, g, b) ( ((r<<8) & 0xF800) | ((g << 3)&0x07E0) | (b>>3) )
#define | RGB8_TO_RGB16(c)

## Typedefs
typedef void(* | InitFunction) (void)
typedef struct SPRITE | SPRITE

## Enumerations
enum | EFontStyle { STYLE_NORMAL, STYLE_BOLD, STYLE_ITALIC }
enum | EFontSize { FONT_SIZE_NORMAL = 0, FONT_SIZE_2X = 1, FONT_SIZE_4X = 2, FONT_SIZE_8X = 3 }

## Detailed Description

Basic structures of nano gfx library

Definition in file nano_gfx_types.h.

## Macro Definition Documentation

## ◆ max

#define max | ( |  | a,
|  |  | b
| ) |  | ((a)>(b)?(a):(b))

Macros returning maximum of 2 numbers

Definition at line 40 of file nano_gfx_types.h.

## ◆ min

#define min | ( |  | a,
|  |  | b
| ) |  | ((a)<(b)?(a):(b))

Macros returning minimum of 2 numbers

Definition at line 35 of file nano_gfx_types.h.

## ◆ RGB8_TO_RGB16

#define RGB8_TO_RGB16 | ( |  | c | ) |

Value:
( (((uint16_t)c & 0b11100000) << 8) | \
(((uint16_t)c & 0b00011100) << 6) | \
(((uint16_t)c & 0b00000011) << 3) )

Macro to convert 3-3-2 color to 5-6-5 color

Definition at line 50 of file nano_gfx_types.h.

## ◆ RGB_COLOR16

#define RGB_COLOR16 | ( |  | r,
|  |  | g,
|  |  | b
| ) |  | ( ((r<<8) & 0xF800) | ((g << 3)&0x07E0) | (b>>3) )

Macro to generate 16-bit color for SSD1351 OLED display

Definition at line 47 of file nano_gfx_types.h.

## ◆ RGB_COLOR8

#define RGB_COLOR8 | ( |  | r,
|  |  | g,
|  |  | b
| ) |  | ( (r & 0xE0) | ((g >> 3)&0x1C) | (b>>6) )

Macro to generate 8-bit color for SSD1331 OLED display

Definition at line 44 of file nano_gfx_types.h.

## Typedef Documentation

## ◆ InitFunction

typedef void(* InitFunction) (void)

Pointer type to LCD display initialization function

Definition at line 55 of file nano_gfx_types.h.

## ◆ SPRITE

typedef struct SPRITE SPRITE

SPRITE structure represents logical graphics object

Deprecated:
  Use NanoSprite or NanoFixedSprite instead.

## Enumeration Type Documentation

## ◆ EFontSize

enum EFontSize

Supported scale font values

Definition at line 66 of file nano_gfx_types.h.

## ◆ EFontStyle

enum EFontStyle

Supported font styles

Definition at line 58 of file nano_gfx_types.h.